microblaze_0
TESTAPP_PERIPHERAL_SOURCES = TestApp_Peripheral/src/TestApp_Peripheral.c TestApp_Peripheral/src/xuartlite_selftest_example.c 
TESTAPP_PERIPHERAL_HEADERS = 
TESTAPP_PERIPHERAL_CC = mb-gcc
TESTAPP_PERIPHERAL_CC_SIZE = mb-size
TESTAPP_PERIPHERAL_CC_OPT = -O2
TESTAPP_PERIPHERAL_CFLAGS = 
TESTAPP_PERIPHERAL_CC_SEARCH = # -B
TESTAPP_PERIPHERAL_LIBPATH = -L./microblaze_0/lib/ # -L
TESTAPP_PERIPHERAL_INCLUDES = -I./microblaze_0/include/ # -I
TESTAPP_PERIPHERAL_LFLAGS = # -l
TESTAPP_PERIPHERAL_CC_PREPROC_FLAG = # -Wp,
TESTAPP_PERIPHERAL_CC_ASM_FLAG = # -Wa,
TESTAPP_PERIPHERAL_CC_LINKER_FLAG = # -Wl,
TESTAPP_PERIPHERAL_LINKER_SCRIPT = TestApp_Peripheral/src/TestApp_Peripheral_LinkScr
TESTAPP_PERIPHERAL_CC_DEBUG_FLAG =  -g 
TESTAPP_PERIPHERAL_CC_GLOBPTR_FLAG= # -mxl-gp-opt
TESTAPP_PERIPHERAL_MODE = executable
TESTAPP_PERIPHERAL_LIBG_OPT = -$(TESTAPP_PERIPHERAL_MODE) microblaze_0
TESTAPP_PERIPHERAL_CC_SOFTMUL_FLAG= -mno-xl-soft-mul 
TESTAPP_PERIPHERAL_CC_START_ADDR_FLAG=  # -Wl,-defsym -Wl,_TEXT_START_ADDR=
TESTAPP_PERIPHERAL_CC_STACK_SIZE_FLAG=  # -Wl,-defsym -Wl,_STACK_SIZE=
                  $(TESTAPP_PERIPHERAL_CC_SOFTMUL_FLAG)  \
