[DisAssemblyWindow]
NumStates=_ 1
State 1=_ 1
[JLinkDriver]
WatchVectorCatch=_ 0
WatchCond=_ 0
Watch0=_ 0 "0x00000000" 0 "0x00000000" 0 "0x00000000" 0 "0x00000000" 0 0 0 0
Watch1=_ 0 "0x00000000" 0 "0x00000000" 0 "0x00000000" 0 "0x00000000" 0 0 0 0
[Low Level]
Pipeline mode=0
Initialized=0
[Disassemble mode]
mode=0
[Breakpoints]
Bp0=_ "Code" "{E:\Dev\FreeRTOS\Source\portable\IAR\STR71x\port.c}.240.4@1" 1 0 0 0 "" 0 ""
Count=1
[Log file]
LoggingEnabled=_ 0
LogFile=_ ""
Category=_ 0
[TermIOLog]
LoggingEnabled=_ 0
LogFile=_ ""
