/*
	FreeRTOS.org V4.1.1 - Copyright (C) 2003-2006 Richard Barry.

	This file is part of the FreeRTOS.org distribution.

	FreeRTOS.org is free software; you can redistribute it and/or modify
	it under the terms of the GNU General Public License as published by
	the Free Software Foundation; either version 2 of the License, or
	(at your option) any later version.

	FreeRTOS.org is distributed in the hope that it will be useful,
	but WITHOUT ANY WARRANTY; without even the implied warranty of
	MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
	GNU General Public License for more details.

	You should have received a copy of the GNU General Public License
	along with FreeRTOS.org; if not, write to the Free Software
	Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA  02111-1307  USA

	A special exception to the GPL can be applied should you wish to distribute
	a combined work that includes FreeRTOS.org, without being obliged to provide
	the source code for any proprietary components.  See the licensing section 
	of http://www.FreeRTOS.org for full details of how and when the exception
	can be applied.

	***************************************************************************
	See http://www.FreeRTOS.org for documentation, latest information, license 
	and contact details.  Please ensure to read the configuration and relevant 
	port sections of the online documentation.
	***************************************************************************
*/

#ifndef PORT_ASM_H
#define PORT_ASM_H

typedef void tskTCB;
extern volatile tskTCB * volatile pxCurrentTCB;
extern void vTaskSwitchContext( void );

/*
 * Saves the stack pointer for one task into its TCB, calls
 * vTaskSwitchContext() to update the TCB being used, then restores the stack
 * from the new TCB read to run the task.
 */
void portSWITCH_CONTEXT( void );

/*
 * Load the stack pointer from the TCB of the task which is going to be first
 * to execute.  Then force an IRET so the registers and IP are popped off the
 * stack.
 */
void portFIRST_CONTEXT( void );

#define portSWITCH_CONTEXT()											\
							asm { mov	bx, [pxCurrentTCB]			}   \
                            asm { mov	word ptr [bx], sp			}	\
							asm { call  far ptr vTaskSwitchContext	}	\
							asm { mov	bx, [pxCurrentTCB]			}	\
							asm { mov	sp, [bx]					}

#define portFIRST_CONTEXT()												\
							asm { mov	bx, [pxCurrentTCB]			}	\
							asm { mov	sp, [bx]					}	\
							asm { pop	bp							}	\
							asm { pop	di							}	\
							asm { pop	si							}	\
   							asm { pop	ds							}	\
   							asm { pop	es							}	\
							asm { pop	dx							}	\
							asm { pop	cx							}	\
							asm { pop	bx							}	\
							asm { pop	ax							}	\
							asm { iret								}


#endif
