/*
	FreeRTOS.org V4.0.3 - Copyright (C) 2003-2006 Richard Barry.

	This file is part of the FreeRTOS.org distribution.

	FreeRTOS.org is free software; you can redistribute it and/or modify
	it under the terms of the GNU General Public License as published by
	the Free Software Foundation; either version 2 of the License, or
	(at your option) any later version.

	FreeRTOS.org is distributed in the hope that it will be useful,
	but WITHOUT ANY WARRANTY; without even the implied warranty of
	MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
	GNU General Public License for more details.

	You should have received a copy of the GNU General Public License
	along with FreeRTOS.org; if not, write to the Free Software
	Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA  02111-1307  USA

	A special exception to the GPL can be applied should you wish to distribute
	a combined work that includes FreeRTOS.org, without being obliged to provide
	the source code for any proprietary components.  See the licensing section
	of http://www.FreeRTOS.org for full details of how and when the exception
	can be applied.

	***************************************************************************
	See http://www.FreeRTOS.org for documentation, latest information, license
	and contact details.  Please ensure to read the configuration and relevant
	port sections of the online documentation.
	***************************************************************************
*/

		RSEG ICODE:CODE
		CODE32

		EXTERN vEMACISR
		PUBLIC vEMACISREntry

; Wrapper for the EMAC interrupt service routine.  This can cause a
; context switch so requires an assembly wrapper.

; Defines the portSAVE_CONTEXT and portRESTORE_CONTEXT macros.
#include "ISR_Support.h"

vEMACISREntry:

	portSAVE_CONTEXT			; Save the context of the current task.

	bl	vEMACISR				; Call the ISR routine.

	portRESTORE_CONTEXT			; Restore the context of the current task -
								; which may be different to the task that
								; was interrupted.

		END

